Pings a target machine.

ping {target string} [-n number]

-   target: string, an IPv4/IPv6 address
-   opts:
    -   n: optional number, how many times to ping

Sends ICMP ping messages to the given target.
Will wait 1 second between pings.